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 From:   C A R  K E M  P R O D U C T S,  I N C.






         4275 St. Johns Parkway






            Sanford, FL 32771







(800) 423-3168





                Emergency phone #: (800) 424-9300 CHEMTREC

To comply with OSHA form #174

SECTION 1 – IDENTIFICATION OF PRODUCT

Product Name:


Glass Cleaner


Product Code:


A-44
Synonym or Cross Reference:
Aerosol Glass Cleaner
SECTION II – HAZARDOUS INGREDIENTS

Ingredients:



CAS No.

TLV

WGT %




Isopropyl Alcohol



67-63-0

2- Butoxyethanol 



111-76-2
Propellants:  Propane


74-98-6

 N-Butane



106-97-8
SECTION III – PHYSICAL DATA

Appearance: 

Slightly cloudy, colorless mist/spray
Vapor Density;

N/E
Odor:


Floral fragrance


Evaporation Rate:

N/E
Specific Gravity

0.986



Solubility In Water:
Complete
Vapor Pressure (mmHg):
N/E



PH:


8.5






Boiling Point:

N/A


Melting Point:

N/A


SECTION IV – FIRE AND EXPLOSION DATA

Flash Point:


No flash by standard methods.
Lower Flammable Limit %:



Upper Flammable Limit %:



Fire Extinguishing Media:

Dry chemical, CO2 or foam is recommended.
Special Fire Fighting Procedures:
CAUTION. Contents under pressure.  Cool exposed containers with water spray to prevent bursting.  

SCBA should be used whenever chemical fires are present.

Unusual Fire and Explosion Hazard:


SECTION V – HEALTH HAZARD / TOXICOLOGICAL PROPERTIES

Acute Effects

Eyes:

May cause mild eye irritation.  Symptoms include stinging, tearing and redness.
Skin:
May cause mild skin irritation.  Prolonged or repeated contact may dry the skin.  Symptoms may include redness, burning, drying of skin and skin burns.
Inhalation:
High vapor/ aerosol concentrations (>1000ppm) are irritating to the respiratory tract.
Ingestion:
May cause headache, dizziness, incoordination, nausea, vomiting, diarrhea and general weakness.


Chronic Effects:
2-Butoxyethanol has caused red blood cell hemolysis in lab animals and secondary injury to the liver and kidneys.  
Carcinogenic:
Yes _ 
No _X
Teratogen:
Yes _
No _

Mutagen:

Yes _
No _

Primary Routes of Exposure:  Skin contact/ absorption, inhalation.
F  I  R  S T  A I D


Inhalation:
Remove to fresh air.  If not breathing, give artificial respiration.  If breathing is difficult, give oxygen.


Skin:

Immediately flush skin with plenty of water for at least 15 minutes while removing contaminated clothing and shoes.  Wash 

clothing before reuse.  Get medical attention immediately. 

Eyes:

Immediately flush eyes with plenty of water for at least 15 minutes.  Get medical attention immediately.

Ingestion:
Seek medical attention immediately.  Call a poison control center or doctor for treatment advice.  Have person sip a glass of 

water if able to swallow.  Never give anything by mouth to an unconscious person.
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                Emergency phone #: (800) 424-9300 CHEMTREC

Product Name: 
A - 44
SECTION VI – REACTIVITY DATA

Stability:



Stable



Conditions To Avoid:

High temperatures
Incompatibility Materials To Avoid:
Acids and strong oxidizers
Hazardous Decomposition Products:
CO, CO2
Hazardous Polymerization:

Will not occur
SECTION VII – SPILL AND DISPOSAL PROCEDURE

Spills, Leak or Release:
Stop all leaks.  Isolate hazard area.  Keep unnecessary and unprotected personnel from entering.  Eliminate all 

ignition sources.  Disperse vapors with water spray.  Prevent runoff from entering drains, sewers, streams or other 

bodies of water.  Absorb spill with inert material.  Absorb unrecoverable product.  Transfer contaminated absorbent, 

soil and other materials to containers for disposal.

Waste Disposal:

Waste must be disposed of in accordance with federal, state and local environmental control regulations.
SECTION VIII – PROTECTION INFORMATION

Respiratory Protection:
When respiratory protection is required use an organic vapor cartridge.  A respiratory program that meets OSHA’s 29 

CFR 1910.34 & ANSI Z88.2 requirements must be followed.
Ventilation:



Protection Gloves:

To prevent repeated or prolonged contact, wear impervious gloves (made from rubber, nitile or neoprene). 
Eye Protection:

Wear safety goggles or glasses.
Other Protective Equip.       

SECTION IX – HANDLING AND STORAGE PRECAUTIONS

Storage and Handling:
Do not use or store near heat, sparks or open flame.  Exposure to temperatures above 120 F may cause bursting.  Do 
not puncture or incinerate containers.  Store in a cool, dry place.  Do not get in eyes, on skin or on clothing.  
Intentional misuse by deliberately concentrating and inhaling may be harmful or fatal.  Keep out of reach of children.

SECTION X – ADDITIONAL INFORMATION

Shipping Information: Please comply with DOT regulations in USA

Hazard Rating:

0 =
Insignificant

Health

1
1 =
Slight


Fire

4


2 =
Moderate


Reactivity
0
3 =
High


Personal Protection B
4 =
Extreme

Product Code:

Prepared on:


This information in the Material Safety Data Sheet has been compiled from our experience and date presented in various technical publications.  

It is the user’s responsibility to determine the suitability of this information for the adoption of the safety precautions s may be necessary. 

We reserve the right to revise Material Safety Data Sheets from time to time as new technical information becomes available.  The user has the responsibility to contact the company to make sure that the sheet is the latest issue.

